
FONGWAH RFCE\_Driver\_ARM.cab is a USB driver for wince 5.0,it patch S8/S3 usb reader.


Install the driver under follow:

1. Copy the cab to wince system files(anywhere).




[PIC-]

1. Run the cab directly.




[PIC-]

1. Choose the directory to install, the directory should be non lost, such as a folder under SD card,refer to 1 in PIC-
2. Edit the directory name (will be creat after installed), click ‘OK’ to install(refer to 2 and 3 in PIC-).



[PIC-]

1. If success, you will find two files named rfusb.dll and usbhid.dll under install directory.



[PIC-]